**1’s and 2’s complement of 8 bit number.**

**Program :**

LDA 3000

CMA

STA 3001

ADI 01

STA 3002

HLT

**Output :**